**CRESTWOOD BOX**

SUGGESTED HED: Contaminants found

Perchloroethylene (PCE)

Ingredient in aerosol dry-cleaning products

EPA safe level: Zero (for water)

Crestwood: 1,300 ppb (soil sample in June 2006)

Vinyl chloride

Breaks down PCE

EPA safe level: Zero

Crestwood: 5.41 ppb (sample from well, May 2016)

NOTE: EPA safe levels are non-enforceable because of the science-based contaminant level established in the 1974 Safe Drinking Water Act

CRESTWOOD MAP

*(InDesign file — copy and paste into your document, change fonts)*

